**HK Audio SI SERIES**

**P10 ceiling mount**

**Tender specifications:**

Pipe bracket for ceiling mounting of speaker systems

Professional tube mount for pan/tilt mounting of up to two professional column speaker systems.

The tube mount shall provide an easily accessible receptacle for the attachment of matching adapter plates, which shall be bolted to the speaker enclosure.

The overall mechanism must allow vertical tilt angles of up to -40° (one speaker) or up to -12.5° (two speakers). In addition, the tube must allow concealed routing of the connecting cable.

**Technical data:**

Mounting type: ceiling mounting

Functional description: easy mounting by hanging and screwing an adapter plate on the speaker with the tube mount; concealed cable routing through the tube

Vertical tilt range: 0° to -40° (1x SI P10x) or 0° to -12.5° (2x SI P10x)

Horizontal swivel range: 90°

Material: steel

Mounting: 4x M8 slotted hole for ceiling mounting

Surface: smooth powder coated (black, white or RAL according to requirements)

Dimensions (H x W x D): 295 x 128 x 166 mm

Weight: 2.3 kg

**Lead product:**

The pipe bracket for ceiling installation of speaker systems shall be the product HK Audio SI SERIES P10 ceiling mount.