**Tender Specification HK Audio BM-360**

Professional ball joint mount for mounting speaker systems on ceilings, walls or surfaces.

The ball joint mount must allow rotation of the connected loudspeaker by 360° on one axis. In addition, the ball joint must also be freely adjustable on a second axis to determine the tilt angle of the loudspeaker. The ball joint mount must ensure a maximum load capacity of 10 kg. The connection is made via an M6 screw.

**Leading brand name:**

The professional ball joint mount for mounting speaker systems on ceilings, walls or surfaces shall be be **HK Audio FINEO BM-360.**

**Technical data:**

Product type: Ball joint wall mount for fixed installation of a loudspeaker system.

Mounting type: Fixed installation on walls, ceilings or surfaces

Material: Steel

Surface: Galvanised and smooth powder-coated (black, white or RAL according to requirements)

Functional description: Mounting of a loudspeaker with possibility of 360° rotation and free angular adjustment by means of a ball joint

Dimensions (W x H x D): 95 x 95 x 142 mm / 3.74 x 3.74 x 5.59 inch

Weight: 0.51 kg / 1.12 lbs