**Tender Specification HK Audio SF-35**

Professional screw-on flange for standard speaker stands with 35 mm tube diameter.

The screw-on flange shall be able to be screwed to a loudspeaker cabinet with a large mounting plate and two slotted holes 9.5 x 26 mm in order to use the loudspeaker either mobile or in a fixed installation with 35 mm stands or wall brackets. A locking screw is provided to ensure a stable connection with anti-twist protection for the loudspeaker.

**Leading brand name:**

The professional screw-on flange for standard speaker stands with 35 mm tube diameter shall be **HK Audio SF-35.**

**Technical data:**

Product type: Screw-on flange for fixed installation or mobile operation on loudspeaker stands

Mounting type: Screw-on flange for loudspeaker enclosures

Material: Steel

Surface: Galvanised and smooth powder-coated (black, white or RAL according to requirements)

Functional description: Screw-on stand sleeve for loudspeakers without internal 35 mm flange, with locking screw

Dimensions (W x H x D): 110 x 104 x 175 mm / 4.33 x 4.09 x 6.89 inch

Weight: 0.70 kg / 1.54 lbs