**Tender Specification HK Audio FINEO FO 12 U-bracket**

Professional U-bracket for mounting speaker systems on ceilings.

The U-bracket must have two lateral hook openings in which the loudspeaker can be hung. The connection to the mounting surface is made via four slotted holes 9 x 8 mm. Lateral rows of holes allow the tilt angle to be adjusted in 10° steps.

For use in sports facilities, certification according to DIN 18032-3 (ball impact resistance) by an independent, accredited testing laboratory must be presented, which also includes the U-bracket as part of the mounting system.

**Leading brand name:**

The professional U-bracket for mounting speaker systems on ceilings and walls shall be **HK Audio FINEO FO 12 U-bracket.**

**Technical data:**

Product type: U-bracket for fixed installation of a loudspeaker system

Mounting type: Fixed installation on ceilings

Material: High-strength steel (S355MC)

Surface: Galvanised and smooth powder-coated (black, white or RAL according to requirements)

Functional description: Easy mounting for one FINEO FO 12 loudspeaker with hook openings and 10° rows of holes for adjusting the tilt angle

Dimensions (W x H x D): 588 x 325 x 100 mm / 23.15 x 12.79 x 3.94 inch

Weight: 1.99 kg / 4.39 lbs