**Tender Specification HK Audio FINEO FO 5 U-bracket**

Professional U-bracket for mounting speaker systems on ceilings and walls.

The U-bracket must have two lateral 6.5 mm slotted holes, which are used to connect to the loudspeaker. The connection to the mounting base is made via four 8 x 5.5 mm slotted holes. A 10 mm hole also allows use on microphone stands or table stands.

For use in sports facilities, certification according to DIN 18032-3 (ball impact resistance) by an independent, accredited testing laboratory must be presented, which also includes the U-bracket as part of the mounting system.

**Leading brand name:**

The professional U-bracket for mounting speaker systems on ceilings and walls shall be **HK Audio FINEO FO 5 U-bracket.**

**Technical data:**

Product type: U-bracket for fixed installation of a loudspeaker system

Mounting type: Fixed installation on walls or ceilings

Material: High-strength steel (S355MC)

Surface: Galvanised and smooth powder-coated (black, white or RAL according to requirements)

Functional description: Easy mounting for one FINEO FO 5 loudspeaker

Dimensions (W x H x D): 202 x 180 x 50 mm / 7.95 x 7.09 x 1.97 inch

Weight: 0.45 kg / 0.99 lbs