**Tender Specification HK Audio FINEO FO S118 F U-bracket**

Professional U-bracket for mounting speaker systems on ceilings.

The U-bracket must have two lateral hook openings in which the loudspeaker can be hung. The connection to the mounting surface is made via four slotted holes 9 x 8 mm. In addition, a slight vertical inclination of the loudspeaker must be adjustable.

For use in sports facilities, certification according to DIN 18032-3 (ball impact resistance) by an independent, accredited testing laboratory must be presented, which also includes the U-bracket as part of the mounting system.

**Leading brand name:**

The professional U-bracket for mounting speaker systems on ceilings shall be **HK Audio FINEO FO S118 F U-bracket.**

**Technical data:**

Product type: U-bracket for fixed installation of a loudspeaker system

Mounting type: Fixed installation on ceilings

Material: High-strength steel (S355MC)

Surface: Galvanised and smooth powder-coated (black, white or RAL according to requirements)

Functional description: Easy mounting for one FINEO FO S118 F loudspeaker with lateral hook openings

Dimensions (W x H x D): 528 x 102 x 200 mm / 20.79 x 4.02 x 7.87 inch

Weight: 2.35 kg / 5.18 lbs