**Tender Specification HK Audio FINEO Swivel & Tilt Mount L (VESA MIS-E)**

Professional swivel and tilt mount for installing larger speaker systems on walls.

The swivel and tilt mount must be able to mount larger loudspeakers weighing up to max. 25 kg on a wall. The loudspeakers mounted in it must be continuously rotatable horizontally and vertically tiltable in 10° steps up to a maximum of 30°. The speakers are mounted using the VESA MIS-E hole pattern (200 x 200 mm). The wall bracket is constructed in two parts and allows the speaker to be hung in a hook opening.

**Leading brand name:**

Professional swivel and tilt mount for mounting larger speaker systems on walls shall be **HK Audio FINEO Swivel & Tilt Mount L (VESA MIS-E).**

**Technical data:**

Product type: Swivel and tilt mount for fixed installation of larger speaker systems up to max. 25 kg weight on walls.

Mounting type: Fixed installation on walls, hole pattern VESA MIS-E (200 x 200 mm)

Material: Steel

Surface: Galvanised and smooth powder-coated (black, white or RAL according to requirements)

Functional description: Mounting of a loudspeaker with possibility of free horizontal alignment and vertical inclination in 10° steps up to max. 30°

Dimensions (W x H x D): 220 x 220 x 106 mm / 8.66 x 8.66 x 4.17 inch

Weight: 2.25 kg / 4.96 lbs