**HK Audio SI SERIES**

**P10 pole mount**

**Tender specifications:**

Bracket for mounting speaker systems on poles, pipes or columns

Professional bracket for mounting speaker systems on poles, pipes or columns.

The pole mount shall be capable of being bolted to the loudspeaker enclosures and shall provide an elongated hole for attachment by means of clamps or similar effective means of attachment.

The overall mechanics must be able to safely support a loudspeaker system, which must be proven by testing and certification of ball impact resistance according to DIN 18032-3.

**Technical data:**

Mounting type: mounting on poles, tubes or columns

Functional description: easy mounting on poles, tubes or columns for 1x P10 each

Tilt range vertical: no tilt possible

Swivel range horizontal: depending on installation situation

Material: steel

Surface: galvanized and smooth powder coated (black, white or RAL according to requirements)

Dimensions (H x W x D): 59 x 86 x 39 mm

Weight: 0.25 kg

**Lead product:**

Bracket for mounting speaker systems on poles, pipes or columns should be the product **HK Audio SI SERIES P10 pole mount.**