**Tender Specification HK Audio FINEO FO 5 Adapter Plate VESA MIS-D**

Professional adapter plate for connecting a ball joint wall mount to a loudspeaker system.

The adapter plate must be conncted to a loudspeaker system with the VESA MIS-D hole pattern (100 x 100 mm). With several punched rows of holes (hole size 9.5 x 7.5 mm), the adapter plate allows a ball joint wall mount to be connected to the loudspeaker system and to maintain the smallest possible wall distance by selecting a suitable hole.

**Leading brand name:**

The professional adapter plate for connecting a ball joint wall mount to a loudspeaker system shall be **HK Audio FINEO FO 5 Adapter Plate VESA MIS-D.**

**Technical data:**

Product type: Adapter plate for connecting a ball joint wall bracket to a loudspeaker system

Mounting type: Fixed installation on walls or ceilings

Material: High-strength steel (S355MC)

Surface: Galvanised and smooth powder-coated (black, white or RAL according to requirements)

Functional description: Mounting by means of VESA MIS-D hole pattern (100 x 100 mm)

Dimensions (W x H x D): 115 x 115 x 8 mm / 4.53 x 4.53 x 0.31 inch

Weight: 0.31 kg / 0.68 lbs